/\* ArduinoBlocks.com \*/

/\* Project: RGB \*/

/\* Author: Rafa Mor \*/

void setup()

{

 pinMode(11, OUTPUT);

pinMode(10, OUTPUT);

pinMode(9, OUTPUT);

}

void loop()

{

 analogWrite(11,255);analogWrite(10,0);analogWrite(9,0);

 delay(1000);

 analogWrite(11,51);analogWrite(10,102);analogWrite(9,255);

 delay(1000);

 analogWrite(11,0);analogWrite(10,153);analogWrite(9,0);

 delay(1000);

}